IFC building model
Schema: "IFC2X3"
File name: "Sample.ifc"
Time stamp: "12/11/2021 3:39:22 PM"
Preprocessor: "IfcOpenShell 0.5.0-dev"
Originating system: "IfcOpenShell 0.5.0-dev"
Application: "Klemen" version "v1.0" by Organization (no name given)

People and organizations
  Person (no name given) of Organization (no name given)
  Owner history of Person (no name given) of Organization (no name given) | application "Klemen" version "v1.0" by Organization (no name given) | change ADDED | created 1636033868 (2021-11-04T13:51:08Z) | last modified by Person (no name given) of Organization (no name given) with "Klemen" version "v1.0" by Organization (no name given)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)

Spatial structure
IFCPROJECT "001601600"
  IFCSITE "Default Site"
    IFCBUILDING "Default Building"
      IFCBUILDINGSTOREY "Default Storey"
        contains 50 elements
          50 x IFCBUILDINGELEMENTPROXY | names: "YZ_Plane", "XZ_Plane", "XY_Plane" (+47 more) | property sets: Basic product data:, Dimensions:, Technical data:, Logistic data:, Manufacturer data:, Contacts:

Property sets
  Basic product data: | properties | on 199 objects (149 (other), 50 IFCBUILDINGELEMENTPROXY)
    Code: = "001601600" (IFCTEXT)
    Name: = "KVR 00" (IFCTEXT)
    Product group: = "ETIBOX Distribution boards, metal enclosures and free-standing cable distribution cabinets" (IFCTEXT)
    Product link: = "https://www.etigroup.eu/products-services/001601600" (IFCTEXT)
    Short description: = "Cable distribution board, KVR 00" (IFCTEXT)
  Dimensions: | properties | on 199 objects (149 (other), 50 IFCBUILDINGELEMENTPROXY)
    Depth (mm): = "320" (IFCTEXT)
    Height (mm): = "780" (IFCTEXT)
    Width (mm): = "400" (IFCTEXT)
  Technical data: | properties | on 199 objects (149 (other), 50 IFCBUILDINGELEMENTPROXY)
    Frequency (Hz): = "/" (IFCTEXT)
    Fusing characteristics: = "/" (IFCTEXT)
    IP Rating: = "IP44" (IFCTEXT)
    Number of poles: = "/" (IFCTEXT)
    Power dissipation (W): = "/" (IFCTEXT)
    Rated current (A): = "/" (IFCTEXT)
    Rated voltage AC (V): = "/" (IFCTEXT)
    Rated voltage DC (V): = "/" (IFCTEXT)
    Voltage type: = "/" (IFCTEXT)
    Weight (kg): = "14.2" (IFCTEXT)
  Logistic data: | properties | on 199 objects (149 (other), 50 IFCBUILDINGELEMENTPROXY)
    Basic packaging: = "1" (IFCTEXT)
    EAN (single product): = "3838895787563" (IFCTEXT)
  Manufacturer data: | properties | on 199 objects (149 (other), 50 IFCBUILDINGELEMENTPROXY)
    City: = "Izlake" (IFCTEXT)
    Country: = "Slovenia" (IFCTEXT)
    Manufacturer: = "ETI Elektroelement d.o.o." (IFCTEXT)
    Postal code: = "1411" (IFCTEXT)
    Street: = "Obrezija 5" (IFCTEXT)
    Website: = "https://www.etigroup.eu/" (IFCTEXT)
  Contacts: | properties | on 199 objects (149 (other), 50 IFCBUILDINGELEMENTPROXY)
    E-mail: = "support@eti.si" (IFCTEXT)
    Fax: = "00386 (0)3 / 56-74-077" (IFCTEXT)
    Telephone: = "00386 (0)3 / 56-57-570" (IFCTEXT)